| The importance of ESD control is getting higher. We can help you to achieve the surface resistivity in the range of 10e7 to 10e10 ohms/sq., of which range was considered to be difficult to control before. Our anti-static agent can solve these problems without contamination by additives. This ion conducive polymer has semi-permanent anti-static is applicable to wide range of resins such as PE, PP, PS, TPE etc. Good dispersion leads to immedate molding after dry blending. >> more
| It is deoxidant with drying performance. It absorbs oxygen, humidity and corrosion gas by chemical reactions. Once gas is absorbed into agents, it cannot come out. It can keep product from deteriorating during transportation. Harzardous substances are not used in our deoxidant. You can throw them away easily into garbage box.

Copyright(C)2014 Thai Meta-Plas Co., Ltd. All Rights Reserved.