Electrically-conducitve forming sheets are widely used for making carrier tape or tray for use of manufacturing line in order to prevent electronic componenets from static electricity interference. Electrically-conductive properties on plastic are realized by special coating technology or compounding technology. Upon customer's requirement, we can offer wide range of thermoforming sheets available.
TRANSPARENT CONDUCTIVE THERMOFORMING A-PET SHEET - TRCL-1060
Decrease environment degration substance by using water soluble conductive ink - Newly developed conductive technology Special electrically-conducive ink realized by nano meter size - Superior electrical properties Surface resistivity is stable by special coating technology even when sheets stretch. - Continuousness Keep stable electrical properties almost semipermanently because of no change of aging deterioration. - Excellent transparency
Application | Trays for electronic components & liquid crystal Carrier tapes
Materials | A-PET
Others | - Surface resistivity : Below 10e6 ohms - Thickness : 0.5mm, 0.7mm. 0.8mm, 1.0mm - Width: 640mm(standard). Complicance with customer's width.
TOP |
TRANSPARENT GREEN COLOR CONDUCTIVE THERMOFORMING A-PET SHEET - SCAP-1060
Increase in productivity. You can check inside parts through transparent green color - Good visibility. - Stable surface resistivity after thermoforming. - Increase in workabilibty - Less outgas. Protect expensive electronic components.
Application | Tray for IC, liquid crystal, electronic components FPC Tray Carrier tape
Materials | A-PET
Others | - Surface resistivity : Below 10e6 ohms - Thickness : From 0.2mm to 1mm - Width: 640mm(standard). Compliance with customer's width.
TOP |
TRANSLUCENT CARBON BLACK CONDUCTIVE THERMOFORMING A-PET SHEET - TRAP-106
Standard conductive thermoforming sheet by carbon black coating - Translucent conductive rigid sheets - Low cost. Dust prevention effect.
Application | Tray for IC, liquid crystal, electronic components FPC Tray Carrier tape
Materials | A-PET
Others | - Surface resistivity : Below 10e6 ohms - Thickness : From 0.2mm to 1mm - Width: 640mm(standard). Complicance with customer's width.
TOP |
CARBON BLACK LOADED CONDUCTIVE SHEETS
We can offer two different thermoforming sheets available upon your requirement. 1. Microme NK (Conductive PS/ABS/Conductive PS) - Excellent Mechanical Properties Microme NK has high strength and stiffness, compared with conventional ABS sheets and performs excellent protective capability as packaging materials such as carrier tapes. Microme NK is almost equivalent to PC sheets. - Good Thermoformability: Microme NK is applicable to wide range of thermoforming temperatures and it is possible to thermoform complicated shapes.
Application | Carrier tapes
Materials | Conductive PS / ABS / Conductive PS
Others | - Surface resistivity : Below 10e6 ohms - Thickness : From 0.2mm to 0.5mm - Width: 640mm
2. Microme PS (Conductive PS/PS/Conductive PS) Carbon black is compounded into surface PS layers. It is more stable surface resistivity level after thermoformed.
Application | Trays for IC, electronic components Carrier tapes
Materials | Conductive PS / PS / Conductive PS
Others | - Surface resistivity : Below 10e6 ohms - Thickness : From 0.3mm to 1.5mm - Width: 640mm
TOP |

Copyright(C)2014 Thai Meta-Plas Co., Ltd. All Rights Reserved.