Cover Tapes for carrier tape are used in the field of SMT process. The stable peeling strength against any materials of carrier tape is quite important to increase production efficiency. Also, electrical properties on cover tapes is needed. In order to meet individual customer's requirements, we offer PSA cover tapes as well as HAA cover tape.
TRANSPARENT CONDUCTIVE PSA COVER TAPE - STN-PSA
With excellent electrically-conducive performance, prevent electronic components from electrostatic charge caused by peeling and friction. It also decreases jumping troubles or electrostatic breakdown of electronic parts. With stable adhesive performance, you can do re-peeling or re-sealing easily. - Use silicone adhesive or acrylic adhesive. Stable sealing strength. Easy re-peeling, re-sealing. - Less haze, good transparency. Check inside electronic parts easily after taping. - Excellent electrically-conducitive performance. Prevent electronic parts from jumping out of carrier tape and electrostatic breakdown
| Width (mm) | Adhesive width (mm) | Length (M)
Silicone Adhesive | 5.4 | 0.8 | 300, 500
9.3 | 1
Acrylic Adhesive | 5.4 | 0.8
9.3 | 1
13.3 | 1.2
21.3 | 1.5
25.5
37.5
TOP |
TRANSPARENT CONDUCTIVE HEAT ACTIVATED COVER TAPE - ST-931
With excellent electrically-conducive performance, prevent semiconductors from electrostatic breakdown and jumping fault. In addition, It has stable pealing strength against embossed carreir tape made from PS, A-PET or PC. It realizes that electronic components are prevented from jumping out of carrier tape under high SMT production line. - Excellent transparency (light transmittance 70%, Haze: 10%) WIth good transparency, you can check inside electronic parts through the cover tape after taping. As a result, it helps workability in product inspection process. - Good sealability against PS, A-PET or PC carrier tape - Excellent conductive performance Surface resistivity : Less than 1.0 x 10e6 ohms WIth special conductive agent, it realizes excellent conductive performance and prevent semiconductors from static electrostatic breakdown or jumping out of carrier tapes.
Thickness | Width | Length | Core in diameter
65 um | 5.5 mm | 300 M 600 M 900 M | 2 inch 3 inch
9.5 mm
13.5 mm
TOP |
TRANSPARENT ANTI-STATIC HEAT ACTIVATED COVER TAPE - AS-931
With stable anti-static performance, prevent semiconductors from electrostatic breakdown and jumping fault. In addition, It has stable pealing strength against embossed carreir tape made from PS, A-PET or PC. It realizes that electronic components are prevented from jumping out of carrier tape under high SMT production line. - Excellent transparency (light transmittance 90%, Haze: 10%) WIth good transparency, you can check inside electronic parts after taping. As a result, it helps workability in product inspection process. - Good sealability against PS, A-PET or PC carrier tape - Excellent anti-static performance WIth special conductive agent, it realizes excellent anti-static performance and prevent semiconductors from electrostatic breakdown or jumping out of carrier tapes.
Thickness | Width | Length | Core in diameter
65 um | 5.5 mm | 300 M 600 M 900 M | 2 inch 3 inch
13.5 mm
21.5 mm
25.5 mm
37.5 mm
TOP |

Copyright(C)2014 Thai Meta-Plas Co., Ltd. All Rights Reserved.