With the expertise of the electrostatic prevention measures,
we lead you to your business success.

2014/2/26 | Thai Meta-Plas Home Page Opened.

| Conductive Forming Sheets Electrically-conductive forming sheets are used for making carrier tapes or trays for manufacturing line to prevent from electronic components damage. Wide range of forming sheets in thickness and width are available. Anti-static Forming Sheets For packaging of electronic components, anti-static properties are necessary. Anti-static packagings realize safety storage/transportation of electronic components. Wide range of forming sheets in thickness/width are available. Heat resistant PP Compounds For food trays use, heat resistant porypropylene compounds are available. In order to heat foods in trays, heat resistant properties are needed. They are also used to make extrusion forming sheets.
| Cover Tapes Cover tapes are used together with carrier tapes for packaging of semiconductors and/or SMT process. We can offer PSA(Pressure Sensitive Adhesive) cover tapes and HAA (Heat Activated Adhesive) cover tapes for your each application.
| Static Dissipative Plates The demand for static dispative plastic plates in manufacturing and R & D facilities increases more than ever. Static dissipative plates have become indispensable in semiconductor, liquid crystal display, electronics, medical, pharmaceutical, food processing precision machinery and biotechnology. To meet customer's each requirement, we can offer wide range of static dissipative or conductive plates made of PVC, A-PET, PETG, PC as well as PMMA. As for fire retardant plastic, FM plates in compliance with FM4910 for clean room materials are available as well.
| TOME-CHAN band "TOME-CHAN" band was developed to package various vegetables, fruits or bread easily. TOME-CHAN is very compact and light weight. Even if you are not powerful, you can pack vegetables into a plastic bags soon. Easy operation! Re-packing is possible.
| Air Absorptive Mat Air Absorptive Mat is a doormat with energy saving, high performance, easy setting and easy maintenance. Air absorption Mat can clean dirt of shoe sole and wheel with spring brushes and air absorption. It is possible to walk in high heels safely.
| Water Wash Shoes Cleaner Dirt and dust attached on the shoe sole are removed easily with water and special spring brushes. All you have to do is walk on Water Wash Shoe Cleaner. It is possible to sterilize the soles of shoes if you use sodium hypochlorite instead of water.
| Ion Conductive agents for PP, PS, PE, Rubber, PU, Acrylic resins The importance of ESD control is getting higher. We can help you to achieve the surface resistivity in the static dissipative range of 10e8 to 10e9 ohms/sq., of which this range was considered to be difficult to control before. This anti-static agent can solve these problems without contamination by additives.

Copyright(C)2014 Thai Meta-Plas Co., Ltd. All Rights Reserved.