Dirt and dust attached on the shoe sole are removed easily with water and special spring brushes. All you have to do is walk on Water Wash Shoe Cleaner. It is possible to sterilize the soles of shoes if you use sodium hypochlorite instead of water.
Uneven surfaces on the soles of shoes are thoroughly cleaned. It is said that about 70 % of dirt and dust to be carried in factories results from attached dirt and dust on the shoe sole of workers. Water Wash Shoe Cleaner can wash uneven area on the soles of work-shoes and work-boots in water with special spring brush mechanism firmly. Only Walking on Shoes Clearner, Shoes Cleaning. With Water Wash Shoe Cleaner set up at the entrance in food factories and precision equipment factories, the cleaning process is done when you walk on it only. Effective sterilizer In the case that you use appropriate doses of sodium hypochlorite as cleaning water, sterilization is possible. |
◆ Specification
Model | PS-1N
Dimension (mm) | A | B | C | D | E
670 | 305 | 830 | 185 | 120
Weight | 80 kg
Material | Main Material : SUS304
Power | AC100V single phase 0.1 kw (AC200V also available)
Control | Start operation at the time of stepping on the plating. The operation time of brushes is set at approx. 10 sec. as default.
TOP |

Copyright(C)2014 Thai Meta-Plas Co., Ltd. All Rights Reserved.